

**Packet Tracer - Verify IPv4 and IPv6 Addressing**

# Addressing Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Device** | **Interface** | **IP Address / Prefix** | | **Default Gateway** |
| R1 | G0/0 | 10.10.1.97 | 255.255.255.224 | N/A |
| *R1*  *R1*  *R1*  *R1* | *G0/0* | 2001:db8:1:1::1/64 | | *N/A* |
| S0/0/1  *S0/0/1*  *S0/0/1* | 10.10.1.6 | 255.255.255.252 | N/A  *N/A*  *N/A* |
| 2001:db8:1:2::2/64 | |
| fe80::1 | |
| R2  *R2*  *R2*  *R2*  *R2* | S0/0/0  *S0/0/0* | 10.10.1.5 | 255.255.255.252 | N/A  *N/A* |
| 2001:db8:1:2::1/64 | |
| S0/0/1  *S0/0/1*  *S0/0/1* | 10.10.1.9 | 255.255.255.252 | N/A  *N/A*  *N/A* |
| 2001:db8:1:3::1/64 | |
| fe80::2 | |
| R3  *R3*  *R3*  *R3*  *R3* | G0/0  *G0/0* | 10.10.1.17 | 255.255.255.240 | N/A  *N/A* |
| 2001:db8:1:4::1/64 | |
| S0/0/1  *S0/0/1*  *S0/0/1* | 10.10.1.10 | 255.255.255.252 | N/A  *N/A*  *N/A* |
| 2001:db8:1:3::2/64 | |
| fe80::3 | |
| PC1  *PC1* | NIC  *NIC* | *blank*10.10.1.100 | *blank*255.255.255.224 | *blank* |
| 2001:DB8:1:1::A | | FE80::1*blank* |
| PC2 | NIC | *blank*10.10.1.20 | *blank*255.255.255.240 | *blank* |
| 2001:DB8:1:4::A | | *blank* |
| *PC2* | *NIC* |  | | *blank*FE80::3 |

*Blank Line, No additional information*

# Objectives

**Part 1: Complete the Addressing Table Documentation**

**Part 2: Test Connectivity Using Ping**

**Part 3: Discover the Path by Tracing the Route**

# Background

Dual-stack allows IPv4 and IPv6 to coexist on the same network. In this activity, you will investigate a dualstack implementation including documenting the IPv4 and IPv6 configuration for end devices, testing connectivity for both IPv4 and IPv6 using **ping**, and tracing the path from end to end for IPv4 and IPv6.Complete the Addressing Table Documentation

**Packet Tracer - Verify IPv4 and IPv6 Addressing**

**Step 1: Use ipconfig to verify IPv4 addressing.**

1. Click **PC1** and open the **Command Prompt.**
2. Enter the **ipconfig /all** command to collect the IPv4 information. Fill-in the **Addressing Table** with the IPv4 address, subnet mask, and default gateway.
3. Click **PC2** and open the **Command Prompt.**
4. Enter the **ipconfig /all** command to collect the IPv4 information. Fill-in the **Addressing Table** with the IPv4 address, subnet mask, and default gateway.

**Step 2: Use ipv6config to verify IPv6 addressing.**

1. On **PC1**, enter the **ipv6config /all** command to collect the IPv6 information. Fill-in the **Addressing Table** with the IPv6 address, subnet prefix, and default gateway.
2. On **PC2**, enter the **ipv6config /all** command to collect the IPv6 information. Fill-in the **Addressing Table** with the IPv6 address, subnet prefix, and default gateway.

## Part 2: Test Connectivity Using Ping

**Step 1: Use ping to verify IPv4 connectivity.**

1. From **PC1**, ping the IPv4 address for **PC2**.

Question:

Was the result successful?

**Yes**

***Type your answers here.***

1. From **PC2**, ping the IPv4 address for **PC1**.

Question:

Was the result successful?

**yes**

***Type your answers here.***

**Step 2: Use ping to verify IPv6 connectivity.**

1. From **PC1**, ping the IPv6 address for **PC2**.

Question:

Was the result successful?

**yes**

***Type your answers here.***

1. From **PC2**, ping the IPv6 address of **PC1**.

Question:

Was the result successful?

**yes**

***Type your answers here.***

## Part 3: Discover the Path by Tracing the Route

**Step 1: Use tracert to discover the IPv4 path.**

1. From **PC1**, trace the route to **PC2**. PC> **tracert 10.10.1.20**

Questions:

What addresses were encountered along the path?

**10.10.1.97, 10.10.1.5, 10.10.1.10, 10.10.1.20*your answers here.***

With which interfaces are the four addresses associated

**G0/0 of R1, S0/0/0 on R2, S0/0/1 on R3, NIC of PC2**

**Packet Tracer - Verify IPv4 and IPv6 Addressing**

1. From **PC2**, trace the route to **PC1**.

Questions:

What addresses were encountered along the path?

**10.10.1.17,**

**10.10.1.9,**

**10.10.1.6,**

**10.10.1.100**

***Type your answers here.***

With which interfaces are the four addresses associated?

**G0/0 of R3,**

**S0/0/1 of R2,**

**S0/0/1 of R1,**

**NIC of PC1**

***Type your answers here.***

**Step 2: Use tracert to discover the IPv6 path.**

1. From **PC1**, trace the route to the IPv6 address for **PC2**.

PC> **tracert 2001:db8:1:4::a**

Questions:

What addresses were encountered along the path?

**2001:db8:1:1::1,**

**2001:db8:1:2::1,**

**2001:db8:1:3::2,**

**2001:db8:1:4::a**

***Type your answers here.***

With which interfaces are the four addresses associated?

**G0/0 of R1,**

**S0/0/0 of r2,**

**S0/0/1 of R3,**

**NIC of PC2**

***Type your answers here.***

1. From **PC2**, trace the route to the IPv6 address for **PC1**.

Questions:

What addresses were encountered along the path?

**2001:db8:1:4::1,**

**2001:db8:1:3::1,**

**2001:db8:1:2::2,**

**2001:db8:1:1::a**

***Type your answers here.***

With which interfaces are the four addresses associated?

**G0/0 of R3,**

**S0/0/1 of R2,**

**S0/0/1 of R1,**

**NIC of PC1**

***Type your answers here.***

*End of document*