Packet Tracer - Basic Router Configuration Review

# Addressing Table

| Device | Interface | IP Address / Prefix | Default Gateway |
| --- | --- | --- | --- |
| R2 | G0/0/0 | 10.0.4.1 /24 | N/A |
| R2 | G0/0/0 | 2001:db8:acad:4::1 /64 | N/A |
| R2 | G0/0/0 | fe80::2:a | N/A |
| R2 | G0/0/1 | 10.0.5.1 /24 | N/A |
| R2 | G0/0/1 | 2001:db8:acad:5::1 /64 | N/A |
| R2 | G0/0/1 | fe80::2:b | N/A |
| R2 | S0/1/0 | 10.0.3.2 /24 | N/A |
| R2 | S0/1/0 | 2001:db8:acad:3::2 /64 | N/A |
| R2 | S0/1/0 | fe80::1:c | N/A |
| R2 | S0/1/1 | 209.165.200.225 /30 | N/A |
| R2 | S0/1/1 | 2001:db8:feed:224::1/64 | N/A |
| R2 | S0/1/1 | fe80::1:d | N/A |
| PC1 | NIC | 10.0.1.10 /24 | 10.0.1.1 |
| PC1 | NIC | 2001:db8:acad:1::10 /64 | fe80::1:a |
| PC2 | NIC | 10.0.2.10 /24 | 10.0.2.1 |
| PC2 | NIC | 2001:db8:acad:2::10 /64 | fe80::1:b |
| PC3 | NIC | 10.0.4.10 /24 | 10.0.4.1 |
| PC-3 | NIC | 2001:db8:acad:4::10 /64 | fe80::2:a |
| PC4 | NIC | 10.0.5.10 /24 | 10.0.5.1 |
| PC-4 | NIC | 2001:db8:acad:5::10 /64 | fe80::2:b |

Blank Line - no additional information

# Objectives

Part 1: Configure Devices and Verify Connectivity

* Assign static IPv4 and IPv6 addresses to the PC interfaces.
* Configure basic router settings.
* Configure the router for SSH.
* Verify network connectivity.

Part 2: Display Router Information

* Retrieve hardware and software information from the router.
* Interpret the startup configuration.
* Interpret the routing table.
* Verify the status of the interfaces.

# Background / Scenario

This activity requires you to configure the **R2** router using the settings from the Addressing Table and the specifications listed. The **R1** router and the devices connected to it have been configured. This is a comprehensive review of previously covered IOS router commands. In Part 1, you will complete basic configurations and interface settings on the router. In Part 2, you will use SSH to connect to the router remotely and utilize the IOS commands to retrieve information from the device to answer questions about the router. For review purposes, this lab provides the commands necessary for specific router configurations.

# Instructions

## Configure Devices and Verify Connectivity

### Configure the PC interfaces.

* + - 1. Configure the IPv4 and IPv6 addresses on PC3 as listed in the Addressing Table.
      2. Configure the IPv4 and IPv6 addresses on PC4 as listed in the Addressing Table.

### Configure the router.

Open configuration window

* + - 1. On the **R2** router, open a terminal. Move to privileged EXEC mode.
      2. Enter configuration mode.
      3. Assign a device name of **R2** to the router.
      4. Configure **c1sco1234** as the encrypted privileged EXEC mode password.
      5. Set the domain name of the router to **ccna-lab.com**.
      6. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
      7. Encrypt the plaintext passwords.
      8. Configure the username **SSHadmin** with an encrypted password of **55Hadm!n**.
      9. Generate a set of crypto keys with a 1024 bit modulus.
      10. Assign **cisco** as the console password, configure sessions to disconnect after six minutes of inactivity, and enable login. To prevent console messages from interrupting commands, use the **logging synchronous** command.
      11. Assign **cisco** as the vty password, configure the vty lines to accept SSH connections only, configure sessions to disconnect after six minutes of inactivity, and enable login using the local database.
      12. Create a banner that warns anyone accessing the device that unauthorized access is prohibited.
      13. Enable IPv6 Routing.
      14. Configure all four interfaces on the router with the IPv4 and IPv6 addressing information from the addressing table above. Configure all four interfaces with descriptions. Activate all four interfaces.
      15. Save the running configuration to the startup configuration file.

Close configuration window

### Verify network connectivity.

* + - 1. Using the command line at **PC3**, ping the IPv4 and IPv6 addresses for **PC4**.

#### Question:

Were the pings successful?

yes

Type your answers here.

* + - 1. From the CLI on **R2** ping the S0/1/1 address of **R1** for both IPv4 and IPv6. The addresses assigned to the S0/1/1 interface on R1 are:

IPv4 address = 10.0.3.1

IPv6 address = 2001:db8:acad:3::1

#### Question:

Were the pings successful?

yes

Type your answers here.

From the command line of **PC3** ping the ISP address 209.165.200.226.

#### Question:

Were the pings successful?

Yes, the PC is using the default gateway router to forward the traffic.Type your answers here.

From **PC3** attempt to ping an address on the ISP for testing, 64.100.1.1.

#### Question:

Were the pings successful?

No, routing has not been configured on the router so only local connected networks are accessible. No default route is set on router R2.Type your answers here.

* + - 1. From the command line of **PC3** open an SSH session to the R2 G0/0/0 IPv4 address and log in as **SSHadmin** with the password **55Hadm!n.**

C:\> **ssh -l SSHadmin 10.0.4.1**

Password:

#### Question:

Was remote access successful?

yes

Type your answers here.

## Display Router Information

In Part 2, you will use **show** commands from an SSH session to retrieve information from the router.

### Establish an SSH session to R2.

From the command line of PC3 open an SSH session to the **R2** G0/0/0 IPv6 address and log in as **SSHadmin** with the password **55Hadm!n**.

### Retrieve important hardware and software information.

Open configuration window

* + - 1. Use the **show version** command to answer questions about the router.

#### Questions:

What is the name of the IOS image that the router is running?

Image version isr4300-universalk9.03.16.05.S.155-3.S5-ext.SPA.bin.

Type your answers here.

How much non-volatile random-access memory (NVRAM) does the router have?

32768K bytes of NVRAM.

Type your answers here.

How much Flash memory does the router have?

3223551K bytes of flash memory.

Type your answers here.

* + - 1. The **show** commands often provide multiple screens of outputs. Filtering the output allows a user to display certain sections of the output. To enable the filtering command, enter a pipe (**|**) character after a **show** command, followed by a filtering parameter and a filtering expression. You can match the output to the filtering statement by using the **include** keyword to display all lines from the output that contain the filtering expression. Filter the **show version** command, using **show version | include register** to answer the following question.

#### Question:

What is the boot process for the router on the next reload?

In most cases (0x2102), the router will undergo a normal boot, load the IOS from the Flash memory, and load the startup configuration from the NVRAM if present. If the config register is 0x2142, the router will bypass the startup config and begin at the user-mode command prompt. If the initial boot fails, the router goes into ROMMON mode.

Type your answers here.

### Display the running configuration.

Use the **show running-config** command on the router to answer the following questions filtering for lines containing the word “password”.

#### Question:

How are passwords presented in the output?

Passwords are encrypted due to the service password-encryption command.

Type your answers here.

Use the **show running-config | begin vty** command.

#### Question:

What is the result of using this command?

A user receives the running configuration output beginning with the line that includes the first instance of the filtering expression.

Type your answers here.

**Note**: A more specific command would be **show running-config | section vty**; however, the current version of Packet Tracer does not support the **section** filtering command.

### Display the routing table on the router.

Use the **show ip route** command on the router to answer the following questions.

#### Question:

What code is used in the routing table to indicate a directly connected network?

The C designates a directly connected subnet. An L designates a local interface. Both answers are correct.

Type your answers here.

How many route entries are coded with a C code in the routing table? 4

Type your answers here.

### Display a summary list of the interfaces on the router.

* + - 1. Use the **show ip interface brief** command on the router to answer the following question.

#### Questions:

What command changed the status of the Gigabit Ethernet ports from administratively down to up?

no shutdown

Type your answers here.

What filtering command would you use to display only the interfaces with addresses assigned?

show ip interface brief | exclude unassigned

Type your answers here.

* + 1. Use the **show ipv6 int brief** command to verify IPv6 settings on R2.

#### Question:

What is the meaning of the [up/up] part of the output?

The [up/up] status reflects the Layer 1 and Layer 2 status of the interface and does not rely on Layer 3 for status.

Type your answers here.

Close configuration window

End of document