Packet Tracer - Verify Directly Connected Networks

# Addressing Table

|  |  |  |  |
| --- | --- | --- | --- |
| Device | Interface | IP Address / Prefix | Default Gateway |
| R1 | G0/0/0 | 172.16.20.1/25 | N/A |
| R1 | G0/0/1 | 172.16.20.129/25 | N/A |
| R1 | S0/1/0 | 209.165.200.225/30 | N/A |
| PC1 | NIC | 172.16.20.10/25 | 172.16.20.1 |
| PC2 | NIC | 172.16.20.138/25 | 172.16.20.129 |
| R2 | G0/0/0 | 2001:db8:c0de:12::1/64 | N/A |
| R2 | G0/0/1 | 2001:db8:c0de:13::1/64 | N/A |
| R2 | S0/1/1 | 2001:db8:c0de:11::1/64 | N/A |
| R2 | S0/1/1 | fe80::2 | N/A |
| PC3 | NIC | 2001:db8:c0de:12::a/64 | fe80::2 |
| PC4 | NIC | 2001:db8:c0de:13::a/64 | fe80::2 |

Blank Line - no additional information

# Objectives

* Verify IPv4 Directly Connected Networks
* Verify IPv6 Directly Connected Networks
* Troubleshoot connectivity issues.

# Background

Routers R1 and R2 each have two LANs. Your task is to verify the addressing on each device and verify connectivity between the LANs.

**Note**: The user EXEC password is **cisco**. The privileged EXEC password is **class**.

# Instructions

## Verify IPv4 Directly Connected Networks

### Verify IPv4 addresses and port status on R1.

* + - 1. Check the status of the configured interfaces by filtering the output.

Open configuration window

R1# **show ip interface brief | exclude unassigned**

* + - 1. Based on the output, correct any port status problems that you see.
      2. Refer to the **Addressing Table** and verify the IP addresses configured on R1. Make any corrections to addressing if necessary.
      3. Display the routing table by filtering to start the output at the word **Gateway**.

**Note:** Terms that are used to filter output can be shortened to match text as long as the match is unique. For example, Gateway, Gate, and Ga will have the same effect. G will not. Filtering is case-sensitive

R1# **show ip route | begin Gate**

#### Question:

What is the Gateway of last resort address?

209.165.200.226

Type your answers here.

* + - 1. Display interface information and filter for **Description** or **connected**.

**Note**: When using **include** or **exclude** multiple searches can be performed by separating the search strings with a pipe symbol ( **|** )

R1# **show interface | include Desc|conn**

#### Question:

What is the Circuit ID displayed from your output?

BCB123450001

Type your answers here.

* + - 1. Display specific interface information for G0/0/0 by filtering for **duplex**.

#### Question:

What is the duplex setting, speed, and media type?

R1#show interfaces gigabitEthernet 0/0/0 | include duplex

Full-duplex, 100Mb/s, media type is RJ45

Type your answers here.

Close configuration window

### Verify connectivity.

**PC1** and **PC2** should be able to ping each other and the **Dual Stack Server**. If not, verify the status of the interfaces and the IP address assignments.

## Verify IPv6 Directly Connected Networks

### Verify IPv6 addresses and port status on R2.

* + - 1. Check the status of the configured interfaces.

Open configuration window

R2# **show ipv6 int brief**

#### Question:

What is the status of the configured interfaces?

2#show ipv6 interface brief

GigabitEthernet0/0/0 [up/up]

FE80::2

2001:DB8:C0DE:12::1

GigabitEthernet0/0/1 [up/up]

FE80::2

2001:DB8:C0DE:14::1

Serial0/1/0 [administratively down/down]

unassigned

Serial0/1/1 [up/up]

FE80::2D0:BCFF:FE32:7C24

2001:DB8:C0DE:11::1

Vlan1 [administratively down/down]

unassigned

R2#

Type your answers here.

* + - 1. Refer to the **Addressing Table** and make any corrections to addressing as necessary.

**Note**: When changing an IPv6 address it is necessary to remove the incorrect address since an interface is capable of supporting multiple IPv6 networks.

R2(config)# **int g0/0/1**

R2(config-if)# **no ipv6 address 2001:db8:c0de:14::1/64**

#### Question:

Configure the correct address on the interface.

R2(config)#int g0/0/1

R2(config-if)#no ipv6 address 2001:DB8:C0DE:14::1/64

R2(config-if)#ipv6 address 2001:db8:c0de:13::1/64

R2(config-if)#exit

R2(config)#int s0/1/1

R2(config-if)#no ipv6 address 2001:DB8:C0DE:11::1/64

R2(config-if)#ipv6 address 2001:db8:c0de:11::1/64

R2(config-if)#

Type your answers here.

* + - 1. Display the IPv6 routing table.

**Note**: Filtering commands do not presently work with the IPv6 commands.

* + - 1. Display all IPv6 addressing configured on interfaces by filtering the output of the **running-config**.

Filter the output on **R2** for **ipv6** or **interface**.

R2# **sh run | include ipv6|interface**

#### Question:

How many addresses are configured on each Gigabit interface?

There are 2 IPv6 addresses. The IPv6 /64 address and the IPv6 link-local address.

Type your answers here.

Close configuration window

### Verify connectivity.

**PC3** and **PC4** should be able to ping each other and the **Dual Stack Server**. If not, verify the interface status and IPv6 address assignments.

End of document